		CONTROL:
			Ethernet/IP is the preferred control method, although RS232 is supported as well.
			
		VIDEO MATRIX:
			The profile supports 16 x 16 video switching, however will default to an 8x8 configuration utilising 2 x PRO-IN4HAB modules and 2 x PRO-OUT4TLS-V2 modules.
			The configuration can be changed through adding, removing or replacing different input and output modules.  The modules that are currently supported are:
			- PRO-IN2HAB
			- PRO-IN4HAB
			- PRO-IN2H2V
			- PRO-OUT4HTCS
			- PRO-OUT4TCS
			- PRO-OUT2TCS
			- PRO-OUT4TL-V2
			- PRO-OUT2TL-V2
			- PRO-OUT4TLS-V2
			- PRO-OUT4H-V2
			- PRO-OUT2H-V2
			
			Each output will be enabled when 1 or more sources are assigned to it and disabled when no sources are assigned to it.
			
		VOLUME CONTROL:
			The profile supports the the basic AV_VOLUMECONTROL_FUNCTION actions, which are:
				IncreaseVolume
				DecreaseVolume
				SetVolume
				MuteOn
				MuteOff
			
		POWER ON/OFF DEVICE:
			A 'PowerOnDevice' custom action and a 'PowerOffDevice' custom action have been added to the profile.
			
		FEEDBACK:
			A number of state variables have been created to provide feedback for each output, these are:
			- Selected Input
			- Current Power Status (Weather the specific output is Enabled or Disabled)
			- Current Mute Status
			- Current Volume
			
			These state variables provide two way feedback.  This means that the state variable values will be updated in the following scenarios:
			A switch(source selection) or volume change for an output is made in Savant
			A switch(source selection) or volume change for an output is made via the Blustream App
			A switch(source selection) or volume change for an output is made via the hard buttons on the matrix (Changes are polled for every 30 seconds)
			
			There is also a Device Power Status state variable (Changes are polled for every 30 seconds) which will provide information on if the device is powered On or Off.
			NOTE: If the device is turned off using the switch on the back of the unit the Device Power Status state variable will not get updated.