		CONTROL:
			Ethernet/IP is the preferred control method, although RS232 is supported as well.

		VIDEO MATRIX:
			The profile supports 32 x 32 HDMI switching, however will default to an 8x8 configuration.
			
			For each Receiver (Output), when a switch action is done a status state variable will be created/updated to show the relevant feedback.
			For example, if OUTPUT 2 is switched to INPUT 1 and INPUT 1 is offline then state variable IP200UHD-OUTPUT_002.SWITCH_STATUS will be updated with "INPUT 001 IS OFFLINE."
			
			A GET_RECIEVER_INFO custom action has also been created for each receiver (Output), which will retrieve the STATUS information of the receiver.