“Toe-in” of screen loudspeakers
•Regardless of whether the screen is curved or not, “toe” the outside loudspeakers inward so that their on-axis extensions intersect at a point 2/3 of the distance to the back wall

| “Toe-in” of screen loudspeakers
| Regardless of whether the screen is curved or not, “toe” the outside loudspeakers inward so that their on-axis extensions intersect at a point 2/3 of the distance to the back wall.