Low frequency driver count
(per “screen” channel)
•For houses with 150 seats or less, specify systems with one LF driver per channel
•
•For houses with 150-to-500 seats, specify systems with two LF drivers per channel
•
•For houses with more than 500 seats, specify systems with four LF drivers per channel

| Low frequency driver count (per “screen” channel)
| For houses with 200 seats or less, specify systems with one LF driver per channel.
| For houses with 200-to-500 seats, specify systems with two LF drivers per channel.
| For houses with more than 500 seats, specify systems with four LF drivers per channel