8340A Surround
•POSITION: True digital power handling capability
•APPLICATION: Surround arrays in digital equipped cinemas
•KEY FEATURES:
–250 watts power handling
–96 dB sensitivity
–THX Approved
4000 Series

| Purely in terms of output capability, irrespective of directional advantages, the 8340 will provide nearly 8 dB more output than the 8330, on a per-unit basis. Most of this capability is used at the frequency extremes in digital effects tracks.
| In many theaters, 8330 surround channels are being retrofitted with the 8340, which has exactly the same mounting requirements. Like the 8330, the 8340’s system response is switchable between flat and rolled off.