3678 Screen Channel System
•POSITION: THX system for small-medium rooms
•APPLICATION: Screen channel in small-medium size cinemas
•KEY FEATURES:
–Shallow profile
–Single VGC 15”
–Bi-Radial horn and medium format driver
–Bi-amp AND Built-in passive network with HF protection
3000 Series

| The 3678 is THX approved for screen channel use In biamp mode for theaters no larger than 3678 cubic meters (45,000 cubic feet), and screen-to-back-row distances no greater than 12.2 meters (40 ft). Key features are its shallow profile, Bi-Radial horn for smooth horizontal and vertical dispersion at high frequencies, and its built-in high frequency driver protection.