5000 Series Technical Attributes
• | Optimized Aperture HF horn/driver design |
| – | 8 - 10 dB lower 2nd harmonic distortion! |
• | Mid-Range horn and driver |
| – | Pattern control |
| – | True mid-range compression driver, model 2490 |
• | VGC 15” LF transducers |
• | Digital Signal Processing |
| – | DSC Family with factory pre-set tunings for 5000 Series
• | Radiation patterns matched at crossover |
| – | Smooth transitions in system power response |
| – | Uniform coverage in the cinema |