•The front-most surrounds are normally 2/3 the distance from the back wall to the screen
•
•The back-most side wall surrounds should be about 9 - 12 feet from the back wall
How to position the surrounds
• Surround density; should be one unit each 9 - 12 feet along the walls

| How to position the surrounds
| The front-most surrounds are normally 2/3 the distance from the back wall to the screen.
| The back-most side wall surrounds should be about 9 - 12 feet from the back wall.