Horizontal “Spacing” of Screen Channel Systems
For a 3-channel (L,C,R) system, L + R speaker channels should be placed |
equidistant from center of screen image area, so that they are just inside the
screen area when screen is masked for the widest format (typically 2.35:1). |
Acoustically |
transparent side |
masking should be |
used to prevent |
blocking of HF |
when side masking
for a “flat” picture |
is moved in |
format. |