JBL ScreenArray®
•3632 ScreenArray® System
•
–Designed for small to medium auditoriums
–Bi-amp or Tri-amp versions available
–3632-T (Tri-amp) is THX- Approved
–30 Hz to 20 kHz frequency range
–129 dB peak SPL
–Multi-band Waveguide

| JBL ScreenArray®
| 3632 ScreenArray® System;
| •Designed for small to medium auditoriums
| •Bi-amp or Tri-amp versions available
| •3632-T (Tri-amp) is THX Approved
| •30 Hz to 20 kHz frequency range
| •129 dB peak SPL
| •Multi-band Waveguide