4632 ScreenArray® System
Designed for medium to large auditoriums
Bi-amp or Tri-amp versions available
4632-T (tri-amp) is THX-Approved
30 Hz to 20 kHz frequency range
135 dB peak SPL
Multi-band Waveguide
4632 ScreenArray

| JBL ScreenArray®
| 4632 ScreenArray® System;
| •Designed for medium to large auditoriums
| •Bi-amp or Tri-amp versions available
| •4632-T (tri-amp) is THX Approved
| •30 Hz to 20 kHz frequency range
| •135 dB peak SPL
| •Multi-band Waveguide