4675C Screen Channel System
•POSITION: Excellent pattern control in an economical passive system
•APPLICATION: Screen channel in medium-large size cinemas
•KEY FEATURES:
–Dual 300 watt 15” woofers
–Large format 2” compression driver
–Large format Bi-Radial horn
–Built-in passive network
4000 Series

| Normally operated via a passive dividing network, the 4675C screen channel system is a natural choice for medium to large theaters in multiplex installations. With a system power rating of 600 watts (IEC noise spectrum) and a sensitivity of 100 dB (one watt at one meter), the 4675C can produce instantaneous peak direct field levels of 102 dB at a distance of 20 meters (66 ft).