Surround channel requirements
•Moderate power surrounds (dome tweeter):
–Sensitivity: 91 dB SPL (1 W at 1 m)
–Power Rating: 100 watts continuous
–
•High power surrounds (compression driver):
–Sensitivity: 96 dB SPL (1 W at 1 m)
–Power Rating: 250 watts continuous
–
•Maximum output difference: 9 dB

| Surround channel requirements;
| Moderate power surrounds (dome tweeter):
| Sensitivity: 91 dB SPL (1 W at 1 m)
| Power Rating: 100 watts continuous
| High power surrounds (compression driver):
| Sensitivity: 96 dB SPL (1 W at 1 m)
| Power Rating: 250 watts continuous
| Maximum output difference: 9 dB