3622N, 2-Way ScreenArray®
•Features:
•JBL 2374 ScreenArray® horn with Screen Spreading Compensation
•JBL 2418H-1, High Frequency Compression Driver
•NEW 3639 Dual 15” Low Frequency System
•Fully Passive Operation utilizing a computer optimized crossover network
•Pre-assembled Components to reduce field assembly time for lower installation cost

| 3622N, 2-Way ScreenArray®
| FEATURES:
| •JBL 2374 ScreenArray® horn with Screen Spreading Compensation
| •JBL 2418H-1, 44mm (1.75in) Diaphragm High Frequency Compression Driver
| •Second Generation Optimized Aperture Waveguide Technology for Ultra Low Distortion and Extremely Low Frequency Response
| •NEW 3639 Dual 15” Low Frequency System
| •Fully Passive Operation utilizing a computer optimized crossover network
| •Pre-assembled Components to reduce field assembly time - lower installation cost