4675C-4(8)LF Screen Channel System
• | POSITION: JBL’s finest two-way THX |
| system |
• | APPLICATION: Screen channel in large
| size cinemas |
• | KEY FEATURES: |
| – | Dual 600 watt VGC 15” woofers |
| – | Large format 2” compression driver |
| – | Large format Bi-Radial horn |
| – | Designed for biampification; available in 4 or 8 ohm
| low frequency impedance for required amplifier |
| matching |