DRIVER_ID			= AUDIO_ZONECTLR_GENDRIVE_SERIAL
DRIVER_NAME			= BlueStream HDMI Zone 7
DRIVER_VERSION		= 1.0 ELAN-generic

BAUD_RATE		= 57600
FLOW_CONTROL		= NONE
PARITY		= NONE
DATA_BITS		= 8
STOP_BITS		= 1
POWER_MODE			= DISCRETE
SOURCE_MODE			= DISCRETE_VERIFY
NUM_SOURCES			= 8

SOURCE_1_NAME	= SOURCE 1
SOURCE_2_NAME	= SOURCE 2
SOURCE_3_NAME	= SOURCE 3
SOURCE_4_NAME	= SOURCE 4
SOURCE_5_NAME	= SOURCE 5
SOURCE_6_NAME	= SOURCE 6
SOURCE_7_NAME	= SOURCE 7
SOURCE_8_NAME	= SOURCE 8

[CODES_BEGIN]
in 1 out 7			= 4F 55 54 20 30 37 20 46 52 20 30 31 0D 
in 2 out 7			= 4F 55 54 20 30 37 20 46 52 20 30 32 0D 
in 3 out 7			= 4F 55 54 20 30 37 20 46 52 20 30 33 0D 
in 4 out 7			= 4F 55 54 20 30 37 20 46 52 20 30 34 0D 
in 5 out 7			= 4F 55 54 20 30 37 20 46 52 20 30 35 0D 
in 6 out 7			= 4F 55 54 20 30 37 20 46 52 20 30 36 0D 
in 7 out 7			= 4F 55 54 20 30 37 20 46 52 20 30 37 0D 
in 8 out 7			= 4F 55 54 20 30 37 20 46 52 20 30 38 0D 
[CODES_END]

[SEQUENCE_START:SOURCE_1]
	SEND_CODE:in 1 out 7
	DELAY:100
[SEQUENCE_END]

[SEQUENCE_START:SOURCE_2]
	SEND_CODE:in 2 out 7
	DELAY:100
[SEQUENCE_END]

[SEQUENCE_START:SOURCE_3]
	SEND_CODE:in 3 out 7
	DELAY:100
[SEQUENCE_END]

[SEQUENCE_START:SOURCE_4]
	SEND_CODE:in 4 out 7
	DELAY:100
[SEQUENCE_END]

[SEQUENCE_START:SOURCE_5]
	SEND_CODE:in 5 out 7
	DELAY:100
[SEQUENCE_END]

[SEQUENCE_START:SOURCE_6]
	SEND_CODE:in 6 out 7
	DELAY:100
[SEQUENCE_END]

[SEQUENCE_START:SOURCE_7]
	SEND_CODE:in 7 out 7
	DELAY:100
[SEQUENCE_END]

[SEQUENCE_START:SOURCE_8]
	SEND_CODE:in 8 out 7
	DELAY:100
[SEQUENCE_END]

[SEQUENCE_START:POWER_OFF]
[SEQUENCE_END]

[SEQUENCE_START:POWER_ON]
	DELAY:18000
[SEQUENCE_END]
[SEQUENCE_START:VOLUME_UP_BEGIN]
[SEQUENCE_END]

[SEQUENCE_START:VOLUME_UP_END]
[SEQUENCE_END]

[SEQUENCE_START:VOLUME_DOWN_BEGIN]
[SEQUENCE_END]

[SEQUENCE_START:VOLUME_DOWN_END]
[SEQUENCE_END]

[SEQUENCE_START:MUTE]
[SEQUENCE_END]
