Placement of Screen Channels
•Space horizontally to match the widest picture format
•Elevate systems so that the HF sections are up about 2/3 the screen height
•Place the systems so that the HF elements are as close as possible to the screen
•Paint matte black any reflecting surfaces

| Placement of screen channels
| Space horizontally to match the widest picture format.
| Elevate systems so that the HF sections are up about 2/3 the screen height.
| Place the systems so that the HF elements are as close as possible to the screen.
| Paint matte black any reflecting surfaces.