•Features:
•JBL 2384 ScreenArray® HF horn with Screen Spreading Compensation
•JBL 2430H, High Frequency Driver
•JBL 4639 Dual 15” Low Frequency System
•Bi-Amplified design
•Pre-assembled Components to reduce field assembly time for lower installation cost
4622, 2-Way ScreenArray®

| 4622, 2-Way ScreenArray ®
| FEATURES:
| •JBL 2384 ScreenArray® HF horn with Screen Spreading Compensation
| •JBL 2430H, 75mm (3 in.) Diaphragm High Frequency compression driver
| •Second Generation Optimized Aperture Waveguide Technology for ultra low distortion
| •JBL 4639 Dual 15” Low Frequency System
| •Bi-Amplified design
| •Pre-assembled Components to reduce field assembly time - lower installation cost